Optical Fiber Network Project
Final Acceptance Test Report
(OSP & IBW Connectivity)


Initial Details
	Project name
	Dialog DE Connections

	Phase
	Phase IV

	Site ID
	CX033107

	Site Name
	INTERNATIONAL COLLEGE OF BUSINESS & TECH LTD

	Site Address
	MAITHRIPALA SENANAYAKE MAWATHA, ANURADHAPURA

	DAP Region
	



Work Completion Details
	JFS date
	13.05.2026

	OSP Completed Date
	23.06.2026

	IBW Completed Date
	23.06.2026

	Splicing & Test Completed Date
	25.06.2026

	Final Acceptance Completed Date (OSP)
	

	Final Acceptance Completed Date (IBW)
	





	Contractor
	Maintenance Team 
	Client

	Name
	Asiri Rasanga
	Name
	 
	Name
	Champika Rathnakantha

	Designation
	A.Engineer
	Designation
	
	Designation
	Engineer

	Date
	 
	Date
	 
	Date
	 

	Signature
	 
	Signature
	 
	Signature
	 




Final Acceptance Test Reports

OSP-Under Ground Method
	Description
	Qty. (m)

	Micro Duct Laying(For 300mm Depth)
	-

	HDPE Duct Laying (For 1m Depth)
	-

	GI Protection (if Applied)
	-

	PVC Protection (if Applied)
	-



	Description
	D1
	D2
	D3
	D4

	Ball Test
	-
	-
	-
	-



OSP-Micro Trenching (MT Method)
	Description
	Depth
	Qty. (m)

	MT(Technology 1 Way)
	-
	-

	MT(Technology 2 Way)
	-
	-

	MT(Technology 4 Way)
	-
	-

	MT(Technology 24 Way)
	-
	-



	Description
	D1
	D2
	D3
	D4

	Ball Test
	-
	-
	-
	-



OSP-Aerial Method
	Description
	Completion

	No of Poles Erection (As per the Drawings)
	-

	Road Crossing for 9m Poles Applied
	-

	No of Struts
	-

	No of Stays
	-

	Well beyond RDA Boundary/SLT Poles & Road Edges
	Done

	Pole Numbering  
	Done





Final Acceptance Test Reports

Installation of Aerial Cables or Under Ground Cable
	Description
	Completion

	Cable Type (As per the As-Built)
	8 Fiber with 4 core tubes

	Cable Distance (Without Coils)
	94.0m

	No of Cable coil Points (500m Intervals)
	-

	No of Splicing Closure Points
	01

	Cable Tagging
	Done

	Cable Earthling (500m Intervals)
	-

	Guard Wire Connectivity to Bulk-Head-Earthling
	Done

	PVC/Flexible Conduits Applied for Unprotect ion Area
	Done



Pre-casted HH/MH installation
	Description
	Completion

	HH/MH & In-Situ Type
	-

	Frame & Cover Fitted
	-

	Brackets
	-

	Earthling
	-

	Duct Entrance
	-

	End Caps
	-

	HH/MH Number
	-



IBW & Connectivity (Site Owner premises & DAP Cabin)
	Description
	Qty. (m)
	Completion

	No of HDPE Duct Laying (Duct No & Colors)
	-
	-

	GI length (Length/Size)
	-
	-

	PVC Length (Length/Size)
	17.9-
	Done

	Flexible Conduits Applied for Unprotecting areas
	4.6
	Done

	Neatness (Color Matching, Tie-wraps)
	 -
	Done

	Bulk-Head sealing
	 -
	-

	ODF Mounted
	 -
	Done

	Inner Wire Grounding 
	 -
	-

	ODF Grounding
	 -
	Done

	ODF Sealing
	 -
	Done

	ODF Labeling (Connected Site & Peer Sites)
	 -
	Done

	Cable Tags
	 -
	Done

	Cable Neatness & Spirals)
	 -
	Done


Standard Formats 
ODF Name (Laminated)
	Connected Site
ICBT Anuradhapura
CX033107



Anuradhapura Suntel
AN0002
G652-8-1-2



ODF Labeling (Connectivity) (Laminated)
	Site East –
Anuradhapura Suntel
AN0002
	Connected Site
ICBT Anuradhapura
CX033107
	Site West –






ICBT Anuradhapura
CX033107
G652-96-17-18

Anuradhapura Suntel
AN0002
G652-8-1-2




Cable Tag-MH-(Stainless Steel_06cmx06cm)				
	Cable Direction to Connected Site







Photographs (Special Locations)
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